<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="QFP80P900X900X120-32N">
</package>
<package name="QFN50P500X500X100-33N">
</package>
<package name="DIP254P762X457-28">
</package>
<package name="TO-92">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03_BORDER">
</package>
<package name="2X03_BORDER_TP">
</package>
<package name="2X03_TP">
</package>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
<package name="RHT03_DHT-22">
<description>&lt;h1&gt;RHT03 / DHT-22&lt;/h1&gt;
&lt;p&gt;
Package for the RHT03 / DHT-22 relative humidity and temperature sensor.
&lt;/p&gt;</description>
</package>
<package name="AM2302">
<description>&lt;h1&gt;AM2302&lt;/h1&gt;
&lt;p&gt;
Package for the AM2302 wired variant of the RHT03/DHT-22 relative humidity and temperature sensor.
&lt;/p&gt;</description>
</package>
<package name="RHT03_DHT-22/RA">
<description>&lt;h1&gt;RHT03 / DHT-22 - RIGHT ANGLE&lt;/h1&gt;
&lt;p&gt;
Right angle package for the RHT03 / DHT-22 relative humidity and temperature sensor.
&lt;/p&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="DIP254P762X533-8">
</package>
<package name="DIP254P762X533-20">
</package>
<package name="SOIC127P798X216-8N">
</package>
<package name="SOIC127P600X175-8N">
</package>
<package name="DIP254P762X508-16">
</package>
<package name="QFP50P1600X1600X120-100N">
</package>
<package name="DIP254P762X508-20">
</package>
<package name="SOIC127P1030X265-20N">
</package>
<package name="DHT11">
</package>
<package name="DHT11-PION.">
</package>
<package name="2X10_BORDER">
</package>
<package name="DIP254P762X508-8">
</package>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
(Motorola)</description>
</package>
<package name="SOT95P270X145-6N">
</package>
<package name="DIP254P1524X482-40">
</package>
<package name="SOP65P640X120-29N">
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOIC-4">
<description>&lt;b&gt;SOIC-4 Package&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/products/discrete/pdf/soic4_dim.pdf</description>
</package>
<package name="USB-B-MICRO-SMD_V03">
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="S4B-PH">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-PCB">
<description>Card-edge USB A connector.

For boards designed to be plugged directly into a USB slot. If possible, ensure that your PCB is about 2.4mm thick to fit snugly.</description>
</package>
<package name="USB-B-PTH-VERTICAL">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S-NOSILK">
</package>
<package name="USB-A-S-NOSILK-FEMALE">
</package>
<package name="USB-MINIB-NOSTOP">
</package>
<package name="USB-A-S-SILK-FEMALE">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="USB-A-SMT-MALE">
</package>
<package name="USB-A-SMT-MALE-LOCKING">
</package>
<package name="CON-HIROSE_ZX62R-B-5P">
<description>&lt;b&gt;MINI USB Connector HI-SPEED Certified&lt;/b&gt; Metal Shield SMT Type Without Positioning Post&lt;p&gt;
Source: http://www.hirose.co.jp/cataloge_hp/e24000019.pdf</description>
</package>
<package name="ISR-PROTOFUSION_POGOPROG-CONN-1H">
<description>Standard pogo pin programming header with ONE alignment hole. Small SMD pads.</description>
</package>
<package name="ISR-PROTOFUSION_POGOPROG-CONN">
<description>Standard pogo pin programming header with two alignment holes. Small SMD pads.</description>
</package>
<package name="ISR-PROTOFUSION_POGOPROG-CONN-W">
<description>Standard pogo pin programming header with two alignment holes. WIDE smd pads.</description>
</package>
<package name="ISR-PROTOFUSION_POGOPROG-CONN-0H">
<description>No holes, 2 vias, pogo pin programming header.</description>
</package>
<package name="ISR-PROTOFUSION_POGOPROG-CONN-OH-1V">
<description>No holes, 1 via, pogo pin programming header.</description>
</package>
<package name="ISR-PROTOFUSION_POGOPROG-CONN-OH-SMALLERVIAS">
<description>No holes, 2 vias, pogo pin programming header. With smaller vias.</description>
</package>
<package name="86SMX">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
<package name="HC13U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC18U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC18U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC33U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC33U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49GW">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49TL-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-LM">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U70">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="MM20SS">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="MM39SL">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="SM49">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC26V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X07/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="PINHEAD_1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="PINHEAD_1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="PINHEAD_2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="PINHEAD_2X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="FPC_0.5MM-4">
</package>
<package name="1X04-BIG">
</package>
<package name="1X04-CLEANBIG">
</package>
<package name="1X04-3.5MM">
</package>
<package name="1X4-SMT">
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X3-SMT">
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X2-SMT">
</package>
<package name="END-LEFT-90-SMT3X">
</package>
<package name="END-RIGHT-90-SMT3X">
</package>
<package name="DIPSWITCH-08">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;
&lt;p&gt;Standard size through-hole DIP switch, 2.54 mm / 0.1" pitch&lt;/p&gt;
Spark Fun Electronics SKU : COM-08034</description>
</package>
<package name="DIPSWITCH-08-50MIL">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;
&lt;p&gt;Half-size SMT DIP switch, 1.27 mm / 0.05" pitch. For example the following:&lt;/p&gt;
&lt;ul&gt;
  &lt;li&gt;Omron A6H series; &lt;a href="http://www.omron.com/ecb/products/pdf/en-a6h.pdf"&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="DIPSWITCH-02">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
<package name="DIPSWITCH-02-50MIL">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;
&lt;p&gt;Half-size SMT DIP switch, 1.27 mm / 0.05" pitch. For example the following:&lt;/p&gt;
&lt;ul&gt;
  &lt;li&gt;A6H-2101 or A6H-2102 in Omron A6H series; &lt;a href="http://www.omron.com/ecb/products/pdf/en-a6h.pdf"&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
  &lt;li&gt;Digikey &lt;a href="http://www.digikey.com/product-detail/en/A6H-2101/A6H-2101-ND/1811590"&gt;A6H-2101-ND&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="SHORT_BOT-50">
<description>Short, bottom layer, 50mil width</description>
</package>
<package name="SHORT_TOP-50">
<description>Short, top layer, 50mil width</description>
</package>
<package name="SHORT_ALL-50">
<description>Short, all layers, 50mil width</description>
</package>
<package name="SHORT_TOP-150">
<description>Short, top layer, 150mil width</description>
</package>
<package name="SHORT_BOT-25">
</package>
</packages>
<symbols>
<symbol name="ATMEGA328P-AU">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="AREF" direction="in"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
</symbol>
<symbol name="ATMEGA328P-MU">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="in"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="EP" direction="pas"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
</symbol>
<symbol name="ATMEGA328P-PU">
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="in"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
</symbol>
<symbol name="1820">
<pin name="VDD" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="DQ" direction="out"/>
</symbol>
<symbol name="ISP-AVR910">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="ATMEGA8L-8PU">
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="in"/>
<pin name="(ICP1)_PB0"/>
<pin name="PB1_(OC1A)"/>
<pin name="PB2_(~SS/OC1B)"/>
<pin name="PB3_(MOSI/OC2)"/>
<pin name="PB4_(MISO)"/>
<pin name="PB5_(SCK)"/>
<pin name="(XTAL1/TOSC1)_PB6" direction="in"/>
<pin name="(XTAL2/TOSC2)_PB7" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PC0_(ADC0)"/>
<pin name="PC1_(ADC1)"/>
<pin name="PC2_(ADC2)"/>
<pin name="PC3_(ADC3)"/>
<pin name="PC4_(ADC4/SDA)"/>
<pin name="PC5_(ADC5/SCL)"/>
<pin name="(RESET)_PC6"/>
<pin name="(RXD)_PD0"/>
<pin name="(TXD)_PD1"/>
<pin name="(INT0)_PD2"/>
<pin name="(INT1)_PD3"/>
<pin name="(XCK/T0)_PD4"/>
<pin name="(T1)_PD5"/>
<pin name="(AIN0)_PD6"/>
<pin name="(AIN1)_PD7"/>
</symbol>
<symbol name="RHT03">
<description>&lt;h1&gt;RHT03 / DHT-22 / AM2302&lt;/h1&gt;
&lt;p&gt;
Symbol for the RHT03 / DHT-22 / AM2302 relative humidity and temperature sensor.
&lt;/p&gt;</description>
<pin name="VDD" direction="pwr"/>
<pin name="DATA"/>
<pin name="NULL" direction="nc"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="74595">
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QH*" direction="hiz"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ATTINY85-20PU">
<pin name="VCC" direction="pwr"/>
<pin name="(PCINT3/XTAL1/CLKI/~OC1B/ADC3)_PB3"/>
<pin name="(PCINT4/XTAL2/CLKO/OC1B/ADC2)_PB4"/>
<pin name="(PCINT5/~RESET/ADC0/DW)_PB5"/>
<pin name="GND" direction="pas"/>
<pin name="PB0_(MOSI/DI/SDA/AIN0/OC0A/~OC1A/AREF/PCINT0)"/>
<pin name="PB1_(MISO/DO/AIN1/OC0B/OC1A/PCINT1)"/>
<pin name="PB2_(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)"/>
</symbol>
<symbol name="ATTINY2313-20PU">
<pin name="VCC" direction="pwr"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="GND" direction="pas"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
</symbol>
<symbol name="ATTINY13-20SU">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
</symbol>
<symbol name="ATTINY13A-PU">
<pin name="VCC" direction="pwr"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="GND" direction="pas"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
</symbol>
<symbol name="ATTINY13A-SSH">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
</symbol>
<symbol name="CD4050BE">
<pin name="VCC" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="VSS" direction="pwr"/>
<pin name="G_=_A" direction="out"/>
<pin name="H_=_B" direction="out"/>
<pin name="I_=_C" direction="out"/>
<pin name="J_=_D" direction="out"/>
<pin name="K_=_E" direction="out"/>
<pin name="L_=_F" direction="out"/>
</symbol>
<symbol name="ATMEGA2560-16AU">
<pin name="AVCC" direction="pwr"/>
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC_3" direction="pwr"/>
<pin name="VCC_4" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="~RESET" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="AREF" direction="in"/>
<pin name="PA0_(AD0)"/>
<pin name="PA1_(AD1)"/>
<pin name="PA2_(AD2)"/>
<pin name="PA3_(AD3)"/>
<pin name="PA4_(AD4)"/>
<pin name="PA5_(AD5)"/>
<pin name="PA6_(AD6)"/>
<pin name="PA7_(AD7)"/>
<pin name="(~SS/PCINT0)_PB0"/>
<pin name="(SCK/PCINT1)_PB1"/>
<pin name="(MOSI/PCINT2)_PB2"/>
<pin name="(MISO/PCINT3)_PB3"/>
<pin name="(OC2A/PCINT4)_PB4"/>
<pin name="(OC1A/PCINT5)_PB5"/>
<pin name="(OC1B/PCINT6)_PB6"/>
<pin name="(OC0A/OC1C/PCINT7)_PB7"/>
<pin name="PC0_(A8)"/>
<pin name="PC1_(A9)"/>
<pin name="PC2_(A10)"/>
<pin name="PC3_(A11)"/>
<pin name="PC4_(A12)"/>
<pin name="PC5_(A13)"/>
<pin name="PC6_(A14)"/>
<pin name="PC7_(A15)"/>
<pin name="(SCL/INT0)_PD0"/>
<pin name="(SDA/INT1)_PD1"/>
<pin name="(RXD1/INT2)_PD2"/>
<pin name="(TXD1/INT3)_PD3"/>
<pin name="(ICP1)_PD4"/>
<pin name="(XCK1)_PD5"/>
<pin name="(T1)_PD6"/>
<pin name="(T0)_PD7"/>
<pin name="(RXD0/PCINT8)_PE0"/>
<pin name="(TXD0)_PE1"/>
<pin name="(XCK0/AIN0)_PE2"/>
<pin name="(OC3A/AIN1)_PE3"/>
<pin name="(OC3B/INT4)_PE4"/>
<pin name="(OC3C/INT5)_PE5"/>
<pin name="(T3/INT6)_PE6"/>
<pin name="(CLKO/ICP3/INT7)_PE7"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND_4" direction="pas"/>
<pin name="GND_5" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="XTAL2" direction="out"/>
<pin name="PF0_(ADC0)"/>
<pin name="PF1_(ADC1)"/>
<pin name="PF2_(ADC2)"/>
<pin name="PF3_(ADC3)"/>
<pin name="PF4_(ADC4/TCK)"/>
<pin name="PF5_(ADC5/TMS)"/>
<pin name="PF6_(ADC6/TDO)"/>
<pin name="PF7_(ADC7/TDI)"/>
<pin name="PG0_(~WR)"/>
<pin name="PG1_(~RD)"/>
<pin name="PG2_(ALE)"/>
<pin name="(TOSC2)_PG3"/>
<pin name="(TOSC1)_PG4"/>
<pin name="(OC0B)_PG5"/>
<pin name="(RXD2)_PH0"/>
<pin name="(TXD2)_PH1"/>
<pin name="(XCK2)_PH2"/>
<pin name="(OC4A)_PH3"/>
<pin name="(OC4B)_PH4"/>
<pin name="(OC4C)_PH5"/>
<pin name="(OC2B)_PH6"/>
<pin name="(T4)_PH7"/>
<pin name="PJ0_(RXD3/PCINT9)"/>
<pin name="PJ1_(TXD3/PCINT10)"/>
<pin name="PJ2_(XCK3/PCINT11)"/>
<pin name="PJ3_(PCINT12)"/>
<pin name="PJ4_(PCINT13)"/>
<pin name="PJ5_(PCINT14)"/>
<pin name="PJ6_(PCINT15)"/>
<pin name="PJ7"/>
<pin name="PK0_(ADC8/PCINT16)"/>
<pin name="PK1_(ADC9/PCINT17)"/>
<pin name="PK2_(ADC10/PCINT18)"/>
<pin name="PK3_(ADC11/PCINT19)"/>
<pin name="PK4_(ADC12/PCINT20)"/>
<pin name="PK5_(ADC13/PCINT21)"/>
<pin name="PK6_(ADC14/PCINT22)"/>
<pin name="PK7_(ADC15/PCINT23)"/>
<pin name="(ICP4)_PL0"/>
<pin name="(ICP5)_PL1"/>
<pin name="(T5)_PL2"/>
<pin name="(OC5A)_PL3"/>
<pin name="(OC5B)_PL4"/>
<pin name="OC5C)_PL5"/>
<pin name="PL6"/>
<pin name="PL7"/>
</symbol>
<symbol name="TPIC6B595N">
<pin name="VCC" direction="pwr"/>
<pin name="RCK" direction="in"/>
<pin name="~SRCLR" direction="in"/>
<pin name="SRCK" direction="in"/>
<pin name="SER_IN" direction="in"/>
<pin name="~G" direction="in"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="DRAIN0" direction="out"/>
<pin name="DRAIN1" direction="out"/>
<pin name="DRAIN2" direction="out"/>
<pin name="DRAIN3" direction="out"/>
<pin name="DRAIN4" direction="out"/>
<pin name="DRAIN5" direction="out"/>
<pin name="DRAIN6" direction="out"/>
<pin name="DRAIN7" direction="out"/>
<pin name="SER_OUT" direction="out"/>
</symbol>
<symbol name="TPIC6B595DW">
<pin name="VCC" direction="pwr"/>
<pin name="~SRCLR" direction="in"/>
<pin name="~G" direction="in"/>
<pin name="RCK" direction="in"/>
<pin name="SRCK" direction="in"/>
<pin name="SER_IN" direction="in"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="DRAIN0" direction="out"/>
<pin name="DRAIN1" direction="out"/>
<pin name="DRAIN2" direction="out"/>
<pin name="DRAIN3" direction="out"/>
<pin name="DRAIN4" direction="out"/>
<pin name="DRAIN5" direction="out"/>
<pin name="DRAIN6" direction="out"/>
<pin name="DRAIN7" direction="out"/>
<pin name="SER_OUT" direction="out"/>
</symbol>
<symbol name="DHT11">
<pin name="VCC"/>
<pin name="DATA"/>
<pin name="NO"/>
<pin name="GND"/>
</symbol>
<symbol name="NE555D">
<pin name="VCC" direction="pwr"/>
<pin name="~RESET" direction="in"/>
<pin name="TRIG" direction="in"/>
<pin name="CONT" direction="pas"/>
<pin name="THRES" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="DISCH" direction="pas"/>
</symbol>
<symbol name="NE555DR">
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="TRIG" direction="in"/>
<pin name="CONT" direction="in"/>
<pin name="THRES" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="DISCH" direction="out"/>
</symbol>
<symbol name="NE555P">
<pin name="VCC" direction="pwr"/>
<pin name="TRIG" direction="in"/>
<pin name="CONT" direction="in"/>
<pin name="THRES" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="DISCH" direction="out"/>
</symbol>
<symbol name="LP2950">
<pin name="I" direction="in"/>
<pin name="O" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MCP3421A1T-E/CH">
<pin name="VDD" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="SDA"/>
</symbol>
<symbol name="ATMEGA8A-AU">
<pin name="VCC_2" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="ADC6" direction="in"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND_3" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PB0" direction="pas"/>
<pin name="PB1" direction="pas"/>
<pin name="PB2" direction="pas"/>
<pin name="PB3" direction="pas"/>
<pin name="PB4" direction="pas"/>
<pin name="PB5" direction="pas"/>
<pin name="PB6"/>
<pin name="PB7" direction="pas"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5" direction="pas"/>
<pin name="PD6" direction="pas"/>
<pin name="PD7" direction="pas"/>
</symbol>
<symbol name="ATMEGA32A-PU">
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="~RESET" direction="in"/>
<pin name="AREF" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="GND_2" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="XTAL2" direction="out"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
</symbol>
<symbol name="TLC5940PWP">
<pin name="VCC" direction="pwr"/>
<pin name="GSCLK" direction="out"/>
<pin name="SCLK" direction="in"/>
<pin name="XLAT" direction="in"/>
<pin name="BLANK" direction="in"/>
<pin name="IREF" direction="in"/>
<pin name="DCPRG" direction="in"/>
<pin name="VPRG" direction="in"/>
<pin name="SIN" direction="in"/>
<pin name="EP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="SOUT" direction="out"/>
<pin name="XERR" direction="out"/>
<pin name="OUT0" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT7" direction="out"/>
<pin name="OUT8" direction="out"/>
<pin name="OUT9" direction="out"/>
<pin name="OUT10" direction="out"/>
<pin name="OUT11" direction="out"/>
<pin name="OUT12" direction="out"/>
<pin name="OUT13" direction="out"/>
<pin name="OUT14" direction="out"/>
<pin name="OUT15" direction="out"/>
</symbol>
<symbol name="139">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="VB" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="pas"/>
</symbol>
<symbol name="CD4046BE">
<pin name="VDD" direction="pwr"/>
<pin name="SIGNAL_IN" direction="in"/>
<pin name="PHASE_PULSES" direction="in"/>
<pin name="ZENER" direction="pas"/>
<pin name="INHIBIT" direction="in"/>
<pin name="C1(1)" direction="in"/>
<pin name="C1(2)" direction="pas"/>
<pin name="VCO_IN" direction="in"/>
<pin name="COMP_IN" direction="in"/>
<pin name="R1_TO_VSS" direction="pas"/>
<pin name="R1_TO_VSS_2" direction="pas"/>
<pin name="VSS" direction="pwr"/>
<pin name="PHASE_COMP_II_OUT" direction="out"/>
<pin name="PHASE_COMP_I_OUT" direction="out"/>
<pin name="DEMODULATION_OUT" direction="out"/>
<pin name="VCO_OUT" direction="out"/>
</symbol>
<symbol name="CD4060BE">
<pin name="VDD" direction="pwr"/>
<pin name="(PHI)O" direction="in"/>
<pin name="~(PHI)O" direction="in"/>
<pin name="(PHI)I" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q4" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q12" direction="out"/>
<pin name="Q13" direction="out"/>
<pin name="Q14" direction="out"/>
</symbol>
<symbol name="CD4040BE">
<pin name="VDD" direction="pwr"/>
<pin name="R" direction="in"/>
<pin name="INPUT_PULSE" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="Q10" direction="out"/>
<pin name="Q11" direction="out"/>
<pin name="Q12" direction="out"/>
</symbol>
<symbol name="OK">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="EMIT" direction="pas"/>
<pin name="COL" direction="pas"/>
</symbol>
<symbol name="OK-TRN">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="DB">
<pin name="AC1" direction="pas"/>
<pin name="+" direction="pas"/>
<pin name="AC2" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="ATTINY85-20SU">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pas"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
</symbol>
<symbol name="MICROB-PLUG">
<pin name="VCC"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="ID"/>
<pin name="GND"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="CON-HIROSE_MINI-USB">
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
</symbol>
<symbol name="ISR-PROTOFUSION_POGOPROG-CONN">
<pin name="GND"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="SCK"/>
<pin name="VCC"/>
<pin name="\RST"/>
</symbol>
<symbol name="Q">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PINHD6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X6">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X7">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHEAD_PINHD4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHEAD_PINH2X4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="1X4">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="SW_DIP-8">
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="SW_DIP-2">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PINHD8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD4">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="PINHD9">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
</symbol>
<symbol name="IGFET-EN-GDS">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="PINHD5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
</symbol>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="+12V">
<pin name="+12V" direction="sup"/>
</symbol>
<symbol name="0V">
<pin name="0V" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="GND_">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="SHORT-H">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="SHORT-V">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="GND1">
<pin name="GND1" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATMEGA328P-AU" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATMEGA328P-AU"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X120-32N">
<connects>
<connect gate="A" pin="ADC6" pad="19"/>
<connect gate="A" pin="ADC7" pad="22"/>
<connect gate="A" pin="AREF" pad="20"/>
<connect gate="A" pin="AVCC" pad="18"/>
<connect gate="A" pin="GND" pad="21"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="PB0" pad="12"/>
<connect gate="A" pin="PB1" pad="13"/>
<connect gate="A" pin="PB2" pad="14"/>
<connect gate="A" pin="PB3" pad="15"/>
<connect gate="A" pin="PB4" pad="16"/>
<connect gate="A" pin="PB5" pad="17"/>
<connect gate="A" pin="PB6" pad="7"/>
<connect gate="A" pin="PB7" pad="8"/>
<connect gate="A" pin="PC0" pad="23"/>
<connect gate="A" pin="PC1" pad="24"/>
<connect gate="A" pin="PC2" pad="25"/>
<connect gate="A" pin="PC3" pad="26"/>
<connect gate="A" pin="PC4" pad="27"/>
<connect gate="A" pin="PC5" pad="28"/>
<connect gate="A" pin="PC6" pad="29"/>
<connect gate="A" pin="PD0" pad="30"/>
<connect gate="A" pin="PD1" pad="31"/>
<connect gate="A" pin="PD2" pad="32"/>
<connect gate="A" pin="PD3" pad="1"/>
<connect gate="A" pin="PD4" pad="2"/>
<connect gate="A" pin="PD5" pad="9"/>
<connect gate="A" pin="PD6" pad="10"/>
<connect gate="A" pin="PD7" pad="11"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VCC_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATMEGA328P-AU"/>
<attribute name="OC_FARNELL" value="1715486"/>
<attribute name="OC_NEWARK" value="14R4631"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA328P-MU" prefix="U">
<description>Programmable Flash</description>
<gates>
<gate name="A" symbol="ATMEGA328P-MU"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X100-33N">
<connects>
<connect gate="A" pin="ADC6" pad="19"/>
<connect gate="A" pin="ADC7" pad="22"/>
<connect gate="A" pin="AREF" pad="20"/>
<connect gate="A" pin="AVCC" pad="18"/>
<connect gate="A" pin="EP" pad="33"/>
<connect gate="A" pin="GND" pad="21"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="PB0" pad="12"/>
<connect gate="A" pin="PB1" pad="13"/>
<connect gate="A" pin="PB2" pad="14"/>
<connect gate="A" pin="PB3" pad="15"/>
<connect gate="A" pin="PB4" pad="16"/>
<connect gate="A" pin="PB5" pad="17"/>
<connect gate="A" pin="PB6" pad="7"/>
<connect gate="A" pin="PB7" pad="8"/>
<connect gate="A" pin="PC0" pad="23"/>
<connect gate="A" pin="PC1" pad="24"/>
<connect gate="A" pin="PC2" pad="25"/>
<connect gate="A" pin="PC3" pad="26"/>
<connect gate="A" pin="PC4" pad="27"/>
<connect gate="A" pin="PC5" pad="28"/>
<connect gate="A" pin="PC6" pad="29"/>
<connect gate="A" pin="PD0" pad="30"/>
<connect gate="A" pin="PD1" pad="31"/>
<connect gate="A" pin="PD2" pad="32"/>
<connect gate="A" pin="PD3" pad="1"/>
<connect gate="A" pin="PD4" pad="2"/>
<connect gate="A" pin="PD5" pad="9"/>
<connect gate="A" pin="PD6" pad="10"/>
<connect gate="A" pin="PD7" pad="11"/>
<connect gate="A" pin="VCC" pad="4"/>
<connect gate="A" pin="VCC_2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATMEGA328P-MU"/>
<attribute name="OC_FARNELL" value="1748522"/>
<attribute name="OC_NEWARK" value="26R2526"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA328P-PU" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATMEGA328P-PU"/>
</gates>
<devices>
<device name="" package="DIP254P762X457-28">
<connects>
<connect gate="A" pin="AREF" pad="21"/>
<connect gate="A" pin="AVCC" pad="20"/>
<connect gate="A" pin="GND" pad="22"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="PB0" pad="14"/>
<connect gate="A" pin="PB1" pad="15"/>
<connect gate="A" pin="PB2" pad="16"/>
<connect gate="A" pin="PB3" pad="17"/>
<connect gate="A" pin="PB4" pad="18"/>
<connect gate="A" pin="PB5" pad="19"/>
<connect gate="A" pin="PB6" pad="9"/>
<connect gate="A" pin="PB7" pad="10"/>
<connect gate="A" pin="PC0" pad="23"/>
<connect gate="A" pin="PC1" pad="24"/>
<connect gate="A" pin="PC2" pad="25"/>
<connect gate="A" pin="PC3" pad="26"/>
<connect gate="A" pin="PC4" pad="27"/>
<connect gate="A" pin="PC5" pad="28"/>
<connect gate="A" pin="PC6" pad="1"/>
<connect gate="A" pin="PD0" pad="2"/>
<connect gate="A" pin="PD1" pad="3"/>
<connect gate="A" pin="PD2" pad="4"/>
<connect gate="A" pin="PD3" pad="5"/>
<connect gate="A" pin="PD4" pad="6"/>
<connect gate="A" pin="PD5" pad="11"/>
<connect gate="A" pin="PD6" pad="12"/>
<connect gate="A" pin="PD7" pad="13"/>
<connect gate="A" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATMEGA328P-PU"/>
<attribute name="OC_FARNELL" value="1715487"/>
<attribute name="OC_NEWARK" value="15R0268"/>
<attribute name="PACKAGE" value="PDIP-28"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1820" prefix="IC">
<description>DS1820 - 1-Wire Digital Thermometer</description>
<gates>
<gate name="G$1" symbol="1820"/>
</gates>
<devices>
<device name="" package="TO-92">
<connects>
<connect gate="G$1" pin="DQ" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICSP" prefix="ISP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="ISP-AVR910"/>
</gates>
<devices>
<device name="PTH" package="2X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="2X03_BORDER">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD_TP" package="2X03_BORDER_TP">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TP" package="2X03_TP">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8L-8PU" prefix="U">
<description>8-bit with 8KBytes In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATMEGA8L-8PU"/>
</gates>
<devices>
<device name="1" package="DIP254P762X457-28">
<connects>
<connect gate="A" pin="(AIN0)_PD6" pad="12"/>
<connect gate="A" pin="(AIN1)_PD7" pad="13"/>
<connect gate="A" pin="(ICP1)_PB0" pad="14"/>
<connect gate="A" pin="(INT0)_PD2" pad="4"/>
<connect gate="A" pin="(INT1)_PD3" pad="5"/>
<connect gate="A" pin="(RESET)_PC6" pad="1"/>
<connect gate="A" pin="(RXD)_PD0" pad="2"/>
<connect gate="A" pin="(T1)_PD5" pad="11"/>
<connect gate="A" pin="(TXD)_PD1" pad="3"/>
<connect gate="A" pin="(XCK/T0)_PD4" pad="6"/>
<connect gate="A" pin="(XTAL1/TOSC1)_PB6" pad="9"/>
<connect gate="A" pin="(XTAL2/TOSC2)_PB7" pad="10"/>
<connect gate="A" pin="AREF" pad="21"/>
<connect gate="A" pin="AVCC" pad="20"/>
<connect gate="A" pin="GND" pad="22"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="PB1_(OC1A)" pad="15"/>
<connect gate="A" pin="PB2_(~SS/OC1B)" pad="16"/>
<connect gate="A" pin="PB3_(MOSI/OC2)" pad="17"/>
<connect gate="A" pin="PB4_(MISO)" pad="18"/>
<connect gate="A" pin="PB5_(SCK)" pad="19"/>
<connect gate="A" pin="PC0_(ADC0)" pad="23"/>
<connect gate="A" pin="PC1_(ADC1)" pad="24"/>
<connect gate="A" pin="PC2_(ADC2)" pad="25"/>
<connect gate="A" pin="PC3_(ADC3)" pad="26"/>
<connect gate="A" pin="PC4_(ADC4/SDA)" pad="27"/>
<connect gate="A" pin="PC5_(ADC5/SCL)" pad="28"/>
<connect gate="A" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="8-bit with 8KBytes In-System Programmable Flash"/>
<attribute name="MPN" value="ATMEGA8L-8PU"/>
<attribute name="OC_FARNELL" value="9171533"/>
<attribute name="OC_NEWARK" value="01M6903"/>
<attribute name="PACKAGE" value="PCDIP-28"/>
<attribute name="SUPPLIER" value="ATMEL"/>
</technology>
</technologies>
</device>
<device name="" package="DIL28-3">
<connects>
<connect gate="A" pin="(AIN0)_PD6" pad="12"/>
<connect gate="A" pin="(AIN1)_PD7" pad="13"/>
<connect gate="A" pin="(ICP1)_PB0" pad="14"/>
<connect gate="A" pin="(INT0)_PD2" pad="4"/>
<connect gate="A" pin="(INT1)_PD3" pad="5"/>
<connect gate="A" pin="(RESET)_PC6" pad="1"/>
<connect gate="A" pin="(RXD)_PD0" pad="2"/>
<connect gate="A" pin="(T1)_PD5" pad="11"/>
<connect gate="A" pin="(TXD)_PD1" pad="3"/>
<connect gate="A" pin="(XCK/T0)_PD4" pad="6"/>
<connect gate="A" pin="(XTAL1/TOSC1)_PB6" pad="9"/>
<connect gate="A" pin="(XTAL2/TOSC2)_PB7" pad="10"/>
<connect gate="A" pin="AREF" pad="21"/>
<connect gate="A" pin="AVCC" pad="20"/>
<connect gate="A" pin="GND" pad="22"/>
<connect gate="A" pin="GND_2" pad="8"/>
<connect gate="A" pin="PB1_(OC1A)" pad="15"/>
<connect gate="A" pin="PB2_(~SS/OC1B)" pad="16"/>
<connect gate="A" pin="PB3_(MOSI/OC2)" pad="17"/>
<connect gate="A" pin="PB4_(MISO)" pad="18"/>
<connect gate="A" pin="PB5_(SCK)" pad="19"/>
<connect gate="A" pin="PC0_(ADC0)" pad="23"/>
<connect gate="A" pin="PC1_(ADC1)" pad="24"/>
<connect gate="A" pin="PC2_(ADC2)" pad="25"/>
<connect gate="A" pin="PC3_(ADC3)" pad="26"/>
<connect gate="A" pin="PC4_(ADC4/SDA)" pad="27"/>
<connect gate="A" pin="PC5_(ADC5/SCL)" pad="28"/>
<connect gate="A" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DHT22_RHT03_DHT-22_AM2302" prefix="U" uservalue="yes">
<description>&lt;h1&gt;RHT03 / DHT-22 / AM2302&lt;/h1&gt;
&lt;p&gt;
Packages and symbol for the RHT03 / DHT-22 relative humidity and temperature sensor.&lt;br /&gt;
Note: The AM2302 is a wired version of the DHT-22 which typically requires less clearance and is thus provided as a separate package.
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RHT03"/>
</gates>
<devices>
<device name="" package="RHT03_DHT-22">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NULL" pad="NULL"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SEN-10167"/>
</technology>
</technologies>
</device>
<device name="WIRED" package="AM2302">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NULL" pad="NULL"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SEN-10167"/>
</technology>
</technologies>
</device>
<device name="RA" package="RHT03_DHT-22/RA">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NULL" pad="NULL"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SEN-10167"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*595" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, output latch</description>
<gates>
<gate name="A" symbol="74595"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="G" pad="17"/>
<connect gate="A" pin="QA" pad="19"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="3"/>
<connect gate="A" pin="QD" pad="4"/>
<connect gate="A" pin="QE" pad="5"/>
<connect gate="A" pin="QF" pad="7"/>
<connect gate="A" pin="QG" pad="8"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="QH*" pad="12"/>
<connect gate="A" pin="RCK" pad="15"/>
<connect gate="A" pin="SCK" pad="14"/>
<connect gate="A" pin="SCL" pad="13"/>
<connect gate="A" pin="SER" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY85-20PU" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATTINY85-20PU"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="(PCINT3/XTAL1/CLKI/~OC1B/ADC3)_PB3" pad="2"/>
<connect gate="A" pin="(PCINT4/XTAL2/CLKO/OC1B/ADC2)_PB4" pad="3"/>
<connect gate="A" pin="(PCINT5/~RESET/ADC0/DW)_PB5" pad="1"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="PB0_(MOSI/DI/SDA/AIN0/OC0A/~OC1A/AREF/PCINT0)" pad="5"/>
<connect gate="A" pin="PB1_(MISO/DO/AIN1/OC0B/OC1A/PCINT1)" pad="6"/>
<connect gate="A" pin="PB2_(SCK/USCK/SCL/ADC1/T0/INT0/PCINT2)" pad="7"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="OC_FARNELL" value="1455162"/>
<attribute name="OC_NEWARK" value="58M3796"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY2313-20PU" prefix="U">
<description>Microcontroller</description>
<gates>
<gate name="A" symbol="ATTINY2313-20PU"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-20">
<connects>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="PA0" pad="5"/>
<connect gate="A" pin="PA1" pad="4"/>
<connect gate="A" pin="PA2" pad="1"/>
<connect gate="A" pin="PB0" pad="12"/>
<connect gate="A" pin="PB1" pad="13"/>
<connect gate="A" pin="PB2" pad="14"/>
<connect gate="A" pin="PB3" pad="15"/>
<connect gate="A" pin="PB4" pad="16"/>
<connect gate="A" pin="PB5" pad="17"/>
<connect gate="A" pin="PB6" pad="18"/>
<connect gate="A" pin="PB7" pad="19"/>
<connect gate="A" pin="PD0" pad="2"/>
<connect gate="A" pin="PD1" pad="3"/>
<connect gate="A" pin="PD2" pad="6"/>
<connect gate="A" pin="PD3" pad="7"/>
<connect gate="A" pin="PD4" pad="8"/>
<connect gate="A" pin="PD5" pad="9"/>
<connect gate="A" pin="PD6" pad="11"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATTINY2313-20PU"/>
<attribute name="OC_FARNELL" value="9171592"/>
<attribute name="OC_NEWARK" value="96K6525"/>
<attribute name="PACKAGE" value="DIP-20"/>
<attribute name="SUPPLIER" value="ATMEL"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY13-20SU" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATTINY13-20SU"/>
</gates>
<devices>
<device name="" package="SOIC127P798X216-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="PB0" pad="5"/>
<connect gate="A" pin="PB1" pad="6"/>
<connect gate="A" pin="PB2" pad="7"/>
<connect gate="A" pin="PB3" pad="2"/>
<connect gate="A" pin="PB4" pad="3"/>
<connect gate="A" pin="PB5" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATTINY13-20SU"/>
<attribute name="OC_FARNELL" value="9171568"/>
<attribute name="OC_NEWARK" value="96K6522"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY13A-PU" prefix="U">
<description>8-bit Microcontroller with 1K Bytes In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATTINY13A-PU"/>
</gates>
<devices>
<device name="" package="DIP254P762X533-8">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="PB0" pad="5"/>
<connect gate="A" pin="PB1" pad="6"/>
<connect gate="A" pin="PB2" pad="7"/>
<connect gate="A" pin="PB3" pad="2"/>
<connect gate="A" pin="PB4" pad="3"/>
<connect gate="A" pin="PB5" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATTINY13A-PU"/>
<attribute name="OC_FARNELL" value="1704566"/>
<attribute name="OC_NEWARK" value="08R5495"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY13A-SSH" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATTINY13A-SSH"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="PB0" pad="5"/>
<connect gate="A" pin="PB1" pad="6"/>
<connect gate="A" pin="PB2" pad="7"/>
<connect gate="A" pin="PB3" pad="2"/>
<connect gate="A" pin="PB4" pad="3"/>
<connect gate="A" pin="PB5" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATTINY13A-SSH"/>
<attribute name="OC_FARNELL" value="1715519"/>
<attribute name="OC_NEWARK" value="15R0301"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CD4050BE" prefix="U">
<description>CMOS Hex Buffer/Converters</description>
<gates>
<gate name="A" symbol="CD4050BE"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="7"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="E" pad="11"/>
<connect gate="A" pin="F" pad="14"/>
<connect gate="A" pin="G_=_A" pad="2"/>
<connect gate="A" pin="H_=_B" pad="4"/>
<connect gate="A" pin="I_=_C" pad="6"/>
<connect gate="A" pin="J_=_D" pad="10"/>
<connect gate="A" pin="K_=_E" pad="12"/>
<connect gate="A" pin="L_=_F" pad="15"/>
<connect gate="A" pin="NC" pad="16"/>
<connect gate="A" pin="NC_2" pad="13"/>
<connect gate="A" pin="VCC" pad="1"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CD4050BE"/>
<attribute name="OC_FARNELL" value="1106108"/>
<attribute name="OC_NEWARK" value="60K5118"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA2560-16AU" prefix="U">
<description>Microcontroller</description>
<gates>
<gate name="A" symbol="ATMEGA2560-16AU"/>
</gates>
<devices>
<device name="" package="QFP50P1600X1600X120-100N">
<connects>
<connect gate="A" pin="(CLKO/ICP3/INT7)_PE7" pad="9"/>
<connect gate="A" pin="(ICP1)_PD4" pad="47"/>
<connect gate="A" pin="(ICP4)_PL0" pad="35"/>
<connect gate="A" pin="(ICP5)_PL1" pad="36"/>
<connect gate="A" pin="(MISO/PCINT3)_PB3" pad="22"/>
<connect gate="A" pin="(MOSI/PCINT2)_PB2" pad="21"/>
<connect gate="A" pin="(OC0A/OC1C/PCINT7)_PB7" pad="26"/>
<connect gate="A" pin="(OC0B)_PG5" pad="1"/>
<connect gate="A" pin="(OC1A/PCINT5)_PB5" pad="24"/>
<connect gate="A" pin="(OC1B/PCINT6)_PB6" pad="25"/>
<connect gate="A" pin="(OC2A/PCINT4)_PB4" pad="23"/>
<connect gate="A" pin="(OC2B)_PH6" pad="18"/>
<connect gate="A" pin="(OC3A/AIN1)_PE3" pad="5"/>
<connect gate="A" pin="(OC3B/INT4)_PE4" pad="6"/>
<connect gate="A" pin="(OC3C/INT5)_PE5" pad="7"/>
<connect gate="A" pin="(OC4A)_PH3" pad="15"/>
<connect gate="A" pin="(OC4B)_PH4" pad="16"/>
<connect gate="A" pin="(OC4C)_PH5" pad="17"/>
<connect gate="A" pin="(OC5A)_PL3" pad="38"/>
<connect gate="A" pin="(OC5B)_PL4" pad="39"/>
<connect gate="A" pin="(RXD0/PCINT8)_PE0" pad="2"/>
<connect gate="A" pin="(RXD1/INT2)_PD2" pad="45"/>
<connect gate="A" pin="(RXD2)_PH0" pad="12"/>
<connect gate="A" pin="(SCK/PCINT1)_PB1" pad="20"/>
<connect gate="A" pin="(SCL/INT0)_PD0" pad="43"/>
<connect gate="A" pin="(SDA/INT1)_PD1" pad="44"/>
<connect gate="A" pin="(T0)_PD7" pad="50"/>
<connect gate="A" pin="(T1)_PD6" pad="49"/>
<connect gate="A" pin="(T3/INT6)_PE6" pad="8"/>
<connect gate="A" pin="(T4)_PH7" pad="27"/>
<connect gate="A" pin="(T5)_PL2" pad="37"/>
<connect gate="A" pin="(TOSC1)_PG4" pad="29"/>
<connect gate="A" pin="(TOSC2)_PG3" pad="28"/>
<connect gate="A" pin="(TXD0)_PE1" pad="3"/>
<connect gate="A" pin="(TXD1/INT3)_PD3" pad="46"/>
<connect gate="A" pin="(TXD2)_PH1" pad="13"/>
<connect gate="A" pin="(XCK0/AIN0)_PE2" pad="4"/>
<connect gate="A" pin="(XCK1)_PD5" pad="48"/>
<connect gate="A" pin="(XCK2)_PH2" pad="14"/>
<connect gate="A" pin="(~SS/PCINT0)_PB0" pad="19"/>
<connect gate="A" pin="AREF" pad="98"/>
<connect gate="A" pin="AVCC" pad="100"/>
<connect gate="A" pin="GND" pad="99"/>
<connect gate="A" pin="GND_2" pad="11"/>
<connect gate="A" pin="GND_3" pad="62"/>
<connect gate="A" pin="GND_4" pad="32"/>
<connect gate="A" pin="GND_5" pad="81"/>
<connect gate="A" pin="OC5C)_PL5" pad="40"/>
<connect gate="A" pin="PA0_(AD0)" pad="78"/>
<connect gate="A" pin="PA1_(AD1)" pad="77"/>
<connect gate="A" pin="PA2_(AD2)" pad="76"/>
<connect gate="A" pin="PA3_(AD3)" pad="75"/>
<connect gate="A" pin="PA4_(AD4)" pad="74"/>
<connect gate="A" pin="PA5_(AD5)" pad="73"/>
<connect gate="A" pin="PA6_(AD6)" pad="72"/>
<connect gate="A" pin="PA7_(AD7)" pad="71"/>
<connect gate="A" pin="PC0_(A8)" pad="53"/>
<connect gate="A" pin="PC1_(A9)" pad="54"/>
<connect gate="A" pin="PC2_(A10)" pad="55"/>
<connect gate="A" pin="PC3_(A11)" pad="56"/>
<connect gate="A" pin="PC4_(A12)" pad="57"/>
<connect gate="A" pin="PC5_(A13)" pad="58"/>
<connect gate="A" pin="PC6_(A14)" pad="59"/>
<connect gate="A" pin="PC7_(A15)" pad="60"/>
<connect gate="A" pin="PF0_(ADC0)" pad="97"/>
<connect gate="A" pin="PF1_(ADC1)" pad="96"/>
<connect gate="A" pin="PF2_(ADC2)" pad="95"/>
<connect gate="A" pin="PF3_(ADC3)" pad="94"/>
<connect gate="A" pin="PF4_(ADC4/TCK)" pad="93"/>
<connect gate="A" pin="PF5_(ADC5/TMS)" pad="92"/>
<connect gate="A" pin="PF6_(ADC6/TDO)" pad="91"/>
<connect gate="A" pin="PF7_(ADC7/TDI)" pad="90"/>
<connect gate="A" pin="PG0_(~WR)" pad="51"/>
<connect gate="A" pin="PG1_(~RD)" pad="52"/>
<connect gate="A" pin="PG2_(ALE)" pad="70"/>
<connect gate="A" pin="PJ0_(RXD3/PCINT9)" pad="63"/>
<connect gate="A" pin="PJ1_(TXD3/PCINT10)" pad="64"/>
<connect gate="A" pin="PJ2_(XCK3/PCINT11)" pad="65"/>
<connect gate="A" pin="PJ3_(PCINT12)" pad="66"/>
<connect gate="A" pin="PJ4_(PCINT13)" pad="67"/>
<connect gate="A" pin="PJ5_(PCINT14)" pad="68"/>
<connect gate="A" pin="PJ6_(PCINT15)" pad="69"/>
<connect gate="A" pin="PJ7" pad="79"/>
<connect gate="A" pin="PK0_(ADC8/PCINT16)" pad="89"/>
<connect gate="A" pin="PK1_(ADC9/PCINT17)" pad="88"/>
<connect gate="A" pin="PK2_(ADC10/PCINT18)" pad="87"/>
<connect gate="A" pin="PK3_(ADC11/PCINT19)" pad="86"/>
<connect gate="A" pin="PK4_(ADC12/PCINT20)" pad="85"/>
<connect gate="A" pin="PK5_(ADC13/PCINT21)" pad="84"/>
<connect gate="A" pin="PK6_(ADC14/PCINT22)" pad="83"/>
<connect gate="A" pin="PK7_(ADC15/PCINT23)" pad="82"/>
<connect gate="A" pin="PL6" pad="41"/>
<connect gate="A" pin="PL7" pad="42"/>
<connect gate="A" pin="VCC" pad="80"/>
<connect gate="A" pin="VCC_2" pad="31"/>
<connect gate="A" pin="VCC_3" pad="10"/>
<connect gate="A" pin="VCC_4" pad="61"/>
<connect gate="A" pin="XTAL1" pad="34"/>
<connect gate="A" pin="XTAL2" pad="33"/>
<connect gate="A" pin="~RESET" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="Microcontroller"/>
<attribute name="MPN" value="ATMEGA2560-16AU"/>
<attribute name="OC_FARNELL" value="1288330"/>
<attribute name="OC_NEWARK" value="23M5051"/>
<attribute name="PACKAGE" value="LQFP-100"/>
<attribute name="SUPPLIER" value="ATMEL"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPIC6B595N" prefix="U">
<description>POWER LOGIC 8-BIT SHIFT REGISTER</description>
<gates>
<gate name="A" symbol="TPIC6B595N"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="DRAIN0" pad="4"/>
<connect gate="A" pin="DRAIN1" pad="5"/>
<connect gate="A" pin="DRAIN2" pad="6"/>
<connect gate="A" pin="DRAIN3" pad="7"/>
<connect gate="A" pin="DRAIN4" pad="14"/>
<connect gate="A" pin="DRAIN5" pad="15"/>
<connect gate="A" pin="DRAIN6" pad="16"/>
<connect gate="A" pin="DRAIN7" pad="17"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="10"/>
<connect gate="A" pin="GND_3" pad="19"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="20"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SER_IN" pad="3"/>
<connect gate="A" pin="SER_OUT" pad="18"/>
<connect gate="A" pin="SRCK" pad="13"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="~G" pad="9"/>
<connect gate="A" pin="~SRCLR" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TPIC6B595N"/>
<attribute name="OC_FARNELL" value="1287675"/>
<attribute name="OC_NEWARK" value="15M1973"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPIC6B595DW" prefix="U">
<description>Power Logic 8-Bit Shift Register</description>
<gates>
<gate name="A" symbol="TPIC6B595DW"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="DRAIN0" pad="4"/>
<connect gate="A" pin="DRAIN1" pad="5"/>
<connect gate="A" pin="DRAIN2" pad="6"/>
<connect gate="A" pin="DRAIN3" pad="7"/>
<connect gate="A" pin="DRAIN4" pad="14"/>
<connect gate="A" pin="DRAIN5" pad="15"/>
<connect gate="A" pin="DRAIN6" pad="16"/>
<connect gate="A" pin="DRAIN7" pad="17"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="19"/>
<connect gate="A" pin="GND_3" pad="10"/>
<connect gate="A" pin="NC" pad="1"/>
<connect gate="A" pin="NC_2" pad="20"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SER_IN" pad="3"/>
<connect gate="A" pin="SER_OUT" pad="18"/>
<connect gate="A" pin="SRCK" pad="13"/>
<connect gate="A" pin="VCC" pad="2"/>
<connect gate="A" pin="~G" pad="9"/>
<connect gate="A" pin="~SRCLR" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TPIC6B595DW"/>
<attribute name="OC_FARNELL" value="1491696"/>
<attribute name="OC_NEWARK" value="52F2783"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DHT11" uservalue="yes">
<description>DHT11 Czujnik temperatury i wilgotności</description>
<gates>
<gate name="G$1" symbol="DHT11"/>
</gates>
<devices>
<device name="" package="DHT11">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NO" pad="NO"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DHT11-PION.">
<description>DHT11 Czujnik temperatury i wilgotności (widok pionowy)</description>
<gates>
<gate name="G$1" symbol="DHT11"/>
</gates>
<devices>
<device name="" package="DHT11-PION.">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NO" pad="NO"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE555D" prefix="U">
<description>PRECISION TIMER</description>
<gates>
<gate name="A" symbol="NE555D"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CONT" pad="5"/>
<connect gate="A" pin="DISCH" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="THRES" pad="6"/>
<connect gate="A" pin="TRIG" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
<connect gate="A" pin="~RESET" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE555D"/>
<attribute name="OC_FARNELL" value="9589880"/>
<attribute name="OC_NEWARK" value="08F2512"/>
<attribute name="PACKAGE" value="8-SOIC"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE555DR" prefix="U">
<description>PRECISION TIMERS</description>
<gates>
<gate name="A" symbol="NE555DR"/>
</gates>
<devices>
<device name="" package="SOIC127P600X175-8N">
<connects>
<connect gate="A" pin="CONT" pad="5"/>
<connect gate="A" pin="DISCH" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="RESET" pad="4"/>
<connect gate="A" pin="THRES" pad="6"/>
<connect gate="A" pin="TRIG" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE555DR"/>
<attribute name="OC_FARNELL" value="7527482"/>
<attribute name="OC_NEWARK" value="75C4440"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE555P" prefix="U">
<description>PRECISION TIMERS</description>
<gates>
<gate name="A" symbol="NE555P"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-8">
<connects>
<connect gate="A" pin="CONT" pad="5"/>
<connect gate="A" pin="DISCH" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="RESET" pad="4"/>
<connect gate="A" pin="THRES" pad="6"/>
<connect gate="A" pin="TRIG" pad="2"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="NE555P"/>
<attribute name="OC_FARNELL" value="9589899"/>
<attribute name="OC_NEWARK" value="60K6706"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2950" prefix="IC">
<description>&lt;b&gt;100 mA, Low Power Low Dropout Voltage Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/LP2950-D.PDF</description>
<gates>
<gate name="G$1" symbol="LP2950"/>
</gates>
<devices>
<device name="Z" package="TO92">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I" pad="3"/>
<connect gate="G$1" pin="O" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="DPACK">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I" pad="1"/>
<connect gate="G$1" pin="O" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP3421A1T-E/CH">
<description>Analog-to-Digital Converter</description>
<gates>
<gate name="A" symbol="MCP3421A1T-E/CH"/>
</gates>
<devices>
<device name="" package="SOT95P270X145-6N">
<connects>
<connect gate="A" pin="SCL" pad="3"/>
<connect gate="A" pin="SDA" pad="4"/>
<connect gate="A" pin="VDD" pad="5"/>
<connect gate="A" pin="VIN+" pad="1"/>
<connect gate="A" pin="VIN-" pad="6"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MCP3421A1T-E/CH"/>
<attribute name="OC_FARNELL" value="1605568"/>
<attribute name="OC_NEWARK" value="11N7998"/>
<attribute name="PACKAGE" value="SOT-6"/>
<attribute name="SUPPLIER" value="Microchip"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8A-AU" prefix="U">
<description>Programmable Flash</description>
<gates>
<gate name="A" symbol="ATMEGA8A-AU"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X120-32N">
<connects>
<connect gate="A" pin="ADC6" pad="19"/>
<connect gate="A" pin="ADC7" pad="22"/>
<connect gate="A" pin="AREF" pad="20"/>
<connect gate="A" pin="AVCC" pad="18"/>
<connect gate="A" pin="GND" pad="21"/>
<connect gate="A" pin="GND_2" pad="3"/>
<connect gate="A" pin="GND_3" pad="5"/>
<connect gate="A" pin="PB0" pad="12"/>
<connect gate="A" pin="PB1" pad="13"/>
<connect gate="A" pin="PB2" pad="14"/>
<connect gate="A" pin="PB3" pad="15"/>
<connect gate="A" pin="PB4" pad="16"/>
<connect gate="A" pin="PB5" pad="17"/>
<connect gate="A" pin="PB6" pad="7"/>
<connect gate="A" pin="PB7" pad="8"/>
<connect gate="A" pin="PC0" pad="23"/>
<connect gate="A" pin="PC1" pad="24"/>
<connect gate="A" pin="PC2" pad="25"/>
<connect gate="A" pin="PC3" pad="26"/>
<connect gate="A" pin="PC4" pad="27"/>
<connect gate="A" pin="PC5" pad="28"/>
<connect gate="A" pin="PC6" pad="29"/>
<connect gate="A" pin="PD0" pad="30"/>
<connect gate="A" pin="PD1" pad="31"/>
<connect gate="A" pin="PD2" pad="32"/>
<connect gate="A" pin="PD3" pad="1"/>
<connect gate="A" pin="PD4" pad="2"/>
<connect gate="A" pin="PD5" pad="9"/>
<connect gate="A" pin="PD6" pad="10"/>
<connect gate="A" pin="PD7" pad="11"/>
<connect gate="A" pin="VCC" pad="6"/>
<connect gate="A" pin="VCC_2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATMEGA8A-AU"/>
<attribute name="OC_FARNELL" value="1748532"/>
<attribute name="OC_NEWARK" value="26R5638"/>
<attribute name="PACKAGE" value="TQFP-32"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32A-PU" prefix="U">
<description>8-bit Microcontrollerwith 32K Bytes In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATMEGA32A-PU"/>
</gates>
<devices>
<device name="" package="DIP254P1524X482-40">
<connects>
<connect gate="A" pin="AREF" pad="32"/>
<connect gate="A" pin="AVCC" pad="30"/>
<connect gate="A" pin="GND" pad="11"/>
<connect gate="A" pin="GND_2" pad="31"/>
<connect gate="A" pin="PA0" pad="40"/>
<connect gate="A" pin="PA1" pad="39"/>
<connect gate="A" pin="PA2" pad="38"/>
<connect gate="A" pin="PA3" pad="37"/>
<connect gate="A" pin="PA4" pad="36"/>
<connect gate="A" pin="PA5" pad="35"/>
<connect gate="A" pin="PA6" pad="34"/>
<connect gate="A" pin="PA7" pad="33"/>
<connect gate="A" pin="PB0" pad="1"/>
<connect gate="A" pin="PB1" pad="2"/>
<connect gate="A" pin="PB2" pad="3"/>
<connect gate="A" pin="PB3" pad="4"/>
<connect gate="A" pin="PB4" pad="5"/>
<connect gate="A" pin="PB5" pad="6"/>
<connect gate="A" pin="PB6" pad="7"/>
<connect gate="A" pin="PB7" pad="8"/>
<connect gate="A" pin="PC0" pad="22"/>
<connect gate="A" pin="PC1" pad="23"/>
<connect gate="A" pin="PC2" pad="24"/>
<connect gate="A" pin="PC3" pad="25"/>
<connect gate="A" pin="PC4" pad="26"/>
<connect gate="A" pin="PC5" pad="27"/>
<connect gate="A" pin="PC6" pad="28"/>
<connect gate="A" pin="PC7" pad="29"/>
<connect gate="A" pin="PD0" pad="14"/>
<connect gate="A" pin="PD1" pad="15"/>
<connect gate="A" pin="PD2" pad="16"/>
<connect gate="A" pin="PD3" pad="17"/>
<connect gate="A" pin="PD4" pad="18"/>
<connect gate="A" pin="PD5" pad="19"/>
<connect gate="A" pin="PD6" pad="20"/>
<connect gate="A" pin="PD7" pad="21"/>
<connect gate="A" pin="VCC" pad="10"/>
<connect gate="A" pin="XTAL1" pad="13"/>
<connect gate="A" pin="XTAL2" pad="12"/>
<connect gate="A" pin="~RESET" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATMEGA32A-PU"/>
<attribute name="OC_FARNELL" value="1704565"/>
<attribute name="OC_NEWARK" value="08R5493"/>
<attribute name="PACKAGE" value="DIP-40"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC5940PWP" prefix="U">
<description>16 CHANNEL LED DRIVER WITH DOT CORRECTION AND GRAYSCALE PWM CONTROL</description>
<gates>
<gate name="A" symbol="TLC5940PWP"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-29N">
<connects>
<connect gate="A" pin="BLANK" pad="2"/>
<connect gate="A" pin="DCPRG" pad="26"/>
<connect gate="A" pin="EP" pad="29"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="GSCLK" pad="25"/>
<connect gate="A" pin="IREF" pad="27"/>
<connect gate="A" pin="OUT0" pad="7"/>
<connect gate="A" pin="OUT1" pad="8"/>
<connect gate="A" pin="OUT10" pad="17"/>
<connect gate="A" pin="OUT11" pad="18"/>
<connect gate="A" pin="OUT12" pad="19"/>
<connect gate="A" pin="OUT13" pad="20"/>
<connect gate="A" pin="OUT14" pad="21"/>
<connect gate="A" pin="OUT15" pad="22"/>
<connect gate="A" pin="OUT2" pad="9"/>
<connect gate="A" pin="OUT3" pad="10"/>
<connect gate="A" pin="OUT4" pad="11"/>
<connect gate="A" pin="OUT5" pad="12"/>
<connect gate="A" pin="OUT6" pad="13"/>
<connect gate="A" pin="OUT7" pad="14"/>
<connect gate="A" pin="OUT8" pad="15"/>
<connect gate="A" pin="OUT9" pad="16"/>
<connect gate="A" pin="SCLK" pad="4"/>
<connect gate="A" pin="SIN" pad="5"/>
<connect gate="A" pin="SOUT" pad="24"/>
<connect gate="A" pin="VCC" pad="28"/>
<connect gate="A" pin="VPRG" pad="6"/>
<connect gate="A" pin="XERR" pad="23"/>
<connect gate="A" pin="XLAT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TLC5940PWP"/>
<attribute name="OC_FARNELL" value="1755256"/>
<attribute name="OC_NEWARK" value="08K4866"/>
<attribute name="PACKAGE" value="HTSSOP-28"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6N139" prefix="OC" uservalue="yes">
<gates>
<gate name="G$1" symbol="139"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VB" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CD4046BE" prefix="U">
<description>CMOS MICROPOWER PHASE LOCKED LOOP</description>
<gates>
<gate name="A" symbol="CD4046BE"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="C1(1)" pad="6"/>
<connect gate="A" pin="C1(2)" pad="7"/>
<connect gate="A" pin="COMP_IN" pad="3"/>
<connect gate="A" pin="DEMODULATION_OUT" pad="10"/>
<connect gate="A" pin="INHIBIT" pad="5"/>
<connect gate="A" pin="PHASE_COMP_II_OUT" pad="13"/>
<connect gate="A" pin="PHASE_COMP_I_OUT" pad="2"/>
<connect gate="A" pin="PHASE_PULSES" pad="1"/>
<connect gate="A" pin="R1_TO_VSS" pad="11"/>
<connect gate="A" pin="R1_TO_VSS_2" pad="12"/>
<connect gate="A" pin="SIGNAL_IN" pad="14"/>
<connect gate="A" pin="VCO_IN" pad="9"/>
<connect gate="A" pin="VCO_OUT" pad="4"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="ZENER" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CD4046BE"/>
<attribute name="OC_FARNELL" value="1106104"/>
<attribute name="OC_NEWARK" value="06F2487"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CD4060BE" prefix="U">
<description>Ripple-carry Binary Counter/Divider and Oscillator</description>
<gates>
<gate name="A" symbol="CD4060BE"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="(PHI)I" pad="11"/>
<connect gate="A" pin="(PHI)O" pad="9"/>
<connect gate="A" pin="Q10" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q13" pad="2"/>
<connect gate="A" pin="Q14" pad="3"/>
<connect gate="A" pin="Q4" pad="7"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="4"/>
<connect gate="A" pin="Q7" pad="6"/>
<connect gate="A" pin="Q8" pad="14"/>
<connect gate="A" pin="Q9" pad="13"/>
<connect gate="A" pin="RESET" pad="12"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
<connect gate="A" pin="~(PHI)O" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CD4060BE"/>
<attribute name="OC_FARNELL" value="1106111"/>
<attribute name="OC_NEWARK" value="60K5122"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CD4040BE" prefix="U">
<description>BINARY COUNTER/DIVIDERS</description>
<gates>
<gate name="A" symbol="CD4040BE"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-16">
<connects>
<connect gate="A" pin="INPUT_PULSE" pad="10"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q10" pad="14"/>
<connect gate="A" pin="Q11" pad="15"/>
<connect gate="A" pin="Q12" pad="1"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="Q5" pad="3"/>
<connect gate="A" pin="Q6" pad="2"/>
<connect gate="A" pin="Q7" pad="4"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="Q9" pad="12"/>
<connect gate="A" pin="R" pad="11"/>
<connect gate="A" pin="VDD" pad="16"/>
<connect gate="A" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CD4040BE"/>
<attribute name="OC_FARNELL" value="1106103"/>
<attribute name="OC_NEWARK" value="60K5112"/>
<attribute name="PACKAGE" value="PDIP-16"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PC817" prefix="OC" uservalue="yes">
<description>&lt;b&gt;SHARP OPTO COUPLER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OK"/>
</gates>
<devices>
<device name="" package="DIL04">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="C" pad="2"/>
<connect gate="A" pin="COL" pad="4"/>
<connect gate="A" pin="EMIT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOC30*M" prefix="OK">
<description>&lt;b&gt;RANDOM-PHASE OPTOISOLATORS TRIAC DRIVER OUTPUT&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com&lt;br&gt;
MOC3020-M.pdf</description>
<gates>
<gate name="-1" symbol="OK-TRN"/>
</gates>
<devices>
<device name="" package="DIL06">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="A1" pad="4"/>
<connect gate="-1" pin="A2" pad="6"/>
<connect gate="-1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name="10">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="MOC3010-M"/>
<attribute name="OC_FARNELL" value="1505423"/>
<attribute name="OC_NEWARK" value="72K8892"/>
</technology>
<technology name="11">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="MOC3011-M"/>
<attribute name="OC_FARNELL" value="1021363"/>
<attribute name="OC_NEWARK" value="72K8893"/>
</technology>
<technology name="12">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="MOC3012-M"/>
<attribute name="OC_FARNELL" value="1021364"/>
<attribute name="OC_NEWARK" value="72K8894"/>
</technology>
<technology name="20">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="MOC3020-M"/>
<attribute name="OC_FARNELL" value="1505425"/>
<attribute name="OC_NEWARK" value="72K8895"/>
</technology>
<technology name="21">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="MOC3021-M"/>
<attribute name="OC_FARNELL" value="1021365"/>
<attribute name="OC_NEWARK" value="95B7895"/>
</technology>
<technology name="22">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="MOC3022-M"/>
<attribute name="OC_FARNELL" value="1021086"/>
<attribute name="OC_NEWARK" value="58K1956"/>
</technology>
<technology name="23">
<attribute name="MF" value="FAIRCHILD SEMICONDUCTOR"/>
<attribute name="MPN" value="MOC3023-M"/>
<attribute name="OC_FARNELL" value="1021367"/>
<attribute name="OC_NEWARK" value="72K8896"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MB*S" prefix="B">
<description>&lt;b&gt;Bridge Rectifier&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/ds/MB/MB6S.pdf</description>
<gates>
<gate name="G$1" symbol="DB"/>
</gates>
<devices>
<device name="" package="SOIC-4">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
<connect gate="G$1" pin="AC1" pad="~1"/>
<connect gate="G$1" pin="AC2" pad="~2"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
<technology name="4"/>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY85-20SU" prefix="U">
<description>8-bit Microcontroller with In-System Programmable Flash</description>
<gates>
<gate name="A" symbol="ATTINY85-20SU"/>
</gates>
<devices>
<device name="" package="SOIC127P798X216-8N">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="PB0" pad="5"/>
<connect gate="A" pin="PB1" pad="6"/>
<connect gate="A" pin="PB2" pad="7"/>
<connect gate="A" pin="PB3" pad="2"/>
<connect gate="A" pin="PB4" pad="3"/>
<connect gate="A" pin="PB5" pad="1"/>
<connect gate="A" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ATTINY85-20SU"/>
<attribute name="OC_FARNELL" value="1455164"/>
<attribute name="OC_NEWARK" value="58M3797"/>
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="JP">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;
&lt;p&gt;USB-B-PTH is fully proven SKU : PRT-00139/CONN-08278
&lt;p&gt;USB-miniB is fully proven SKU : PRT-00587
&lt;p&gt;USB-A-PCB is untested.
&lt;p&gt;USB-A-H is throughly reviewed, but untested. Spark Fun Electronics SKU : PRT-00437
&lt;p&gt;USB-B-SMT is throughly reviewed, but untested. Needs silkscreen touching up.
&lt;p&gt;USB-A-S has not been used/tested
&lt;p&gt;USB-MB-H has not been used/tested
&lt;P&gt;USB-MICROB has been used. CONN-09505</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D-"/>
<connect gate="G$1" pin="D-" pad="D+"/>
<connect gate="G$1" pin="GND" pad="VBUS"/>
<connect gate="G$1" pin="VBUS" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-S" package="USB-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OLD" package="USB-MINIB-OLD">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08278"/>
<attribute name="VALUE" value="USB-B"/>
</technology>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S4B-PH">
<connects>
<connect gate="G$1" pin="D+" pad="2"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VBUS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08193"/>
</technology>
</technologies>
</device>
<device name="PCB" package="USB-A-PCB">
<connects>
<connect gate="G$1" pin="D+" pad="USB_P"/>
<connect gate="G$1" pin="D-" pad="USB_M"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="5V"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-VERTICAL" package="USB-B-PTH-VERTICAL">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-A-S-NOSILK" package="USB-A-S-NOSILK">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-SMD" package="USB-A-S-NOSILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09520"/>
</technology>
</technologies>
</device>
<device name="-SMD-NS" package="USB-MINIB-NOSTOP">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="USB-A-S-SILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICROB" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND MT1 MT2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09505"/>
</technology>
</technologies>
</device>
<device name="A-SMD-MALE" package="USB-A-SMT-MALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+1"/>
<connect gate="G$1" pin="D-" pad="D-1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="VBUS" pad="VBUS1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A-SMD-MALE-LOCKING" package="USB-A-SMT-MALE-LOCKING">
<connects>
<connect gate="G$1" pin="D+" pad="D+1"/>
<connect gate="G$1" pin="D-" pad="D-1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="VBUS" pad="VBUS1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-HIROSE_MICRO-USB-">
<description>&lt;p&gt;&lt;b&gt;Hirose Micro USB Connector&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;
&lt;ul&gt;&lt;li&gt;ZX62R-B-5P: Micro B, reverse (top mount) shell SMT&lt;br&gt;
Supplier: DigiKey H11574CT-ND&lt;/li&gt;&lt;/ul&gt;
&lt;/p&gt;
&lt;p&gt;Source: http://www.hirose.co.jp/cataloge_hp/e24200011.pdf&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CON-HIROSE_MINI-USB"/>
</gates>
<devices>
<device name="ZX62R-B-5P" package="CON-HIROSE_ZX62R-B-5P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISR-PROTOFUSION_POGOPIN-CONN">
<description>Protofusion custom pogo pin programming header</description>
<gates>
<gate name="J" symbol="ISR-PROTOFUSION_POGOPROG-CONN"/>
</gates>
<devices>
<device name="ONEHOLE" package="ISR-PROTOFUSION_POGOPROG-CONN-1H">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="STANDARD" package="ISR-PROTOFUSION_POGOPROG-CONN">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="ISR-PROTOFUSION_POGOPROG-CONN-W">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHVIAS" package="ISR-PROTOFUSION_POGOPROG-CONN-0H">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHVIAS-1V" package="ISR-PROTOFUSION_POGOPROG-CONN-OH-1V">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WITHVIAS-SMV" package="ISR-PROTOFUSION_POGOPROG-CONN-OH-SMALLERVIAS">
<connects>
<connect gate="J" pin="GND" pad="5"/>
<connect gate="J" pin="MISO" pad="3"/>
<connect gate="J" pin="MOSI" pad="2"/>
<connect gate="J" pin="SCK" pad="4"/>
<connect gate="J" pin="VCC" pad="6"/>
<connect gate="J" pin="\RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL" prefix="Q" uservalue="yes">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="68SMX" package="86SMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="6344860"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="CTS406" package="CTS406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC13U-H" package="HC13U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC18U-H" package="HC18U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC18U-V" package="HC18U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC33U-H" package="HC33U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC33U-V" package="HC33U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49GW" package="HC49GW">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49S" package="HC49/S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49TL-H" package="HC49TL-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49U-H" package="HC49U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1666973"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49U-LM" package="HC49U-LM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1666956"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49U-V" package="HC49U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1666969"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49U70" package="HC49U70">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="HC49UP" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="MM20SS" package="MM20SS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="MM39SL" package="MM39SL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SM49" package="SM49">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TC26H" package="TC26H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TC26V" package="TC26V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="TC38H" package="TC38H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD6"/>
</gates>
<devices>
<device name="" package="1X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X03/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X4"/>
</gates>
<devices>
<device name="" package="2X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X04/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X6" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X6"/>
</gates>
<devices>
<device name="" package="2X06">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X06/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X7" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X7"/>
</gates>
<devices>
<device name="" package="2X07">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X07/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHEAD_PINHD-1X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHEAD_PINHD4"/>
</gates>
<devices>
<device name="" package="PINHEAD_1X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="PINHEAD_1X04/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHEAD_PINHD-2X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHEAD_PINH2X4"/>
</gates>
<devices>
<device name="" package="PINHEAD_2X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="PINHEAD_2X04/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1X4" prefix="CN">
<description>4-pin connector</description>
<gates>
<gate name="G$1" symbol="1X4"/>
</gates>
<devices>
<device name="FPC0.5" package="FPC_0.5MM-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-BIG" package="1X04-BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CLEANBIG" package="1X04-CLEANBIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3.5MM" package="1X04-3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT" package="1X4-SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X3" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="1" package="1X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X03/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X3-SMT">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="0" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X02/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X2-SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="END-LEFT-90-SMT3X-DEV">
<gates>
<gate name="G$1" symbol="PINHD3"/>
</gates>
<devices>
<device name="" package="END-LEFT-90-SMT3X">
<connects>
<connect gate="G$1" pin="1" pad="GND1 GND2"/>
<connect gate="G$1" pin="2" pad="IN1 IN2 IN3"/>
<connect gate="G$1" pin="3" pad="VCC1 VCC2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_DIP-8" prefix="SW" uservalue="yes">
<description>&lt;b&gt;DIP Switch 8 Position&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SW_DIP-8"/>
</gates>
<devices>
<device name="" package="DIPSWITCH-08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMT-HALFSIZE" package="DIPSWITCH-08-50MIL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_DIP-2" prefix="SW" uservalue="yes">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SW_DIP-2"/>
</gates>
<devices>
<device name="" package="DIPSWITCH-02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMT-HALFSIZE" package="DIPSWITCH-02-50MIL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X8" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD8"/>
</gates>
<devices>
<device name="" package="1X08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X08/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X4" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD4"/>
</gates>
<devices>
<device name="" package="1X04">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X04/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X9" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD9"/>
</gates>
<devices>
<device name="" package="1X09">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X09/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF540" prefix="Q">
<description>&lt;b&gt;N-Channel Enhancement MOSFET&lt;/b&gt; (HEXFET); 100V; 28A; 0,077Ohm</description>
<gates>
<gate name="G$1" symbol="IGFET-EN-GDS"/>
</gates>
<devices>
<device name="" package="TO220">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-1X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD5"/>
</gates>
<devices>
<device name="" package="1X05">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="1X05/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V" prefix="V">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+12V" prefix="V">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+12V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0V" prefix="V">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="0V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND_" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;&lt;p&gt;
Net GND, no value text label</description>
<gates>
<gate name="G$1" symbol="GND_"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SHORT-H" prefix="SH">
<description>Short between two nets</description>
<gates>
<gate name="G$1" symbol="SHORT-H"/>
</gates>
<devices>
<device name="B5" package="SHORT_BOT-50">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="no"/>
</technology>
</technologies>
</device>
<device name="T5" package="SHORT_TOP-50">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="no"/>
</technology>
</technologies>
</device>
<device name="A5" package="SHORT_ALL-50">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="no"/>
</technology>
</technologies>
</device>
<device name="C" package="SHORT_TOP-150">
<connects>
<connect gate="G$1" pin="P$1" pad="L"/>
<connect gate="G$1" pin="P$2" pad="R"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="no"/>
</technology>
</technologies>
</device>
<device name="SOR" package="SHORT_BOT-25">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SHORT-V" prefix="SH">
<description>Short between two nets</description>
<gates>
<gate name="G$1" symbol="SHORT-V"/>
</gates>
<devices>
<device name="B5" package="SHORT_BOT-50">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="no"/>
</technology>
</technologies>
</device>
<device name="T5" package="SHORT_TOP-50">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="no"/>
</technology>
</technologies>
</device>
<device name="A5" package="SHORT_ALL-50">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="no"/>
</technology>
</technologies>
</device>
<device name="C" package="SHORT_TOP-150">
<connects>
<connect gate="G$1" pin="P$1" pad="L"/>
<connect gate="G$1" pin="P$2" pad="R"/>
</connects>
<technologies>
<technology name="">
<attribute name="BOM" value="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND1" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="GND1"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
